;* Title:       Block Copy Routines
;* Version:     1.1

.include "8515def.inc"

        rjmp    RESET       ;reset handle

.def    flashsize=r16       ;size of block to be copied

flash2ram:
        lpm                 ;get constant
        st      Y+,r0       ;store in SRAM and increment Y-pointer
        adiw    ZL,1        ;increment Z-pointer
        dec     flashsize
        brne    flash2ram   ;if not end of table, loop more
        ret

.def    ramtemp =r1         ;temporary storage register
.def    ramsize =r16        ;size of block to be copied
